XFcBtClientWin.h File Reference

Main Page Class Hierarchy Alphabetical List Compound List File List Compound Members File Members

# XFcBtClientWin.h File Reference

Include dependency graph for XFcBtClientWin.h:

## Compounds

class | XFcBtClientWin
| Holds bluetooth client data that is used to keep up data flow from/to server. More...

## Enumerations

enum

XFCNET_BT_LINESTATUS {
XFCNET_BT_LINESTATUS_DISCONNECT = -1,
XFCNET_BT_LINESTATUS_FAILED = -2,
XFCNET_BT_LINESTATUS_CONNECTING = -3,
XFCNET_BT_LINESTATUS_OK = 1,
XFCNET_BT_LINESTATUS_CANCEL = -4,
XFCNET_BT_LINESTATUS_WAIT = -5,
XFCNET_BT_LINESTATUS_ONHOLD = -6
}

| Holds bluetooth line status. More...

## Variables

const UINT32 | XFCNET_QUEUE_BUFFER_SIZE = 128
| Size of the buffer allocated for packet (MTU).
const UINT32 | XFCNET_QUEUE_BUFFER_COUNT = 10
| Granularity of queue.

## Enumeration Type Documentation

enum XFCNET_BT_LINESTATUS

Holds bluetooth line status.

Enumeration values:

  XFCNET_BT_LINESTATUS_DISCONNECT | Socket disconnected.
  XFCNET_BT_LINESTATUS_FAILED | Connection failed.
  XFCNET_BT_LINESTATUS_CONNECTING | Socket connecting to server.
  XFCNET_BT_LINESTATUS_OK | Socket connected to server.
  XFCNET_BT_LINESTATUS_CANCEL | Socket connection canceled.
  XFCNET_BT_LINESTATUS_WAIT | Socket waits client to connect.
  XFCNET_BT_LINESTATUS_ONHOLD | Socket connected but not accepted.

## Variable Documentation

const UINT32 XFCNET_QUEUE_BUFFER_COUNT = 10`[static]`

| Granularity of queue.

const UINT32 XFCNET_QUEUE_BUFFER_SIZE = 128`[static]`

| Size of the buffer allocated for packet (MTU).

|  | X-Forge Documentation Confidential Copyright © 2002-2003 Fathammer |  | Documentation generated with doxygen by Dimitri van Heesch